Lipo Cells

We strongly recommend setting this item manually instead of using the default setting “Auto Calculation (which means calculating the LiPo cells automatically)”. The ESC can identify 2S, 4S and 6S LiPo packs when setting this item to “Auto Calculation”. After you power on the ESC, if the battery voltage is below 8.8V, it will be identified as a 2S; if the voltage is from 8.8V to 17.6V, it will be identified as a 4S; if the voltage is above 17.6V, and it will be identified as a 6S.

Note:

You need to set this item to “Auto Calculation.” when you use a NiMH pack or a 5S LiPo, AND customize the "Low Voltage Cutoff" threshold.