Lipo Cells

We strongly recommend setting this item manually instead of using the defaul t setting “Auto Calc. (which means calculating the LiPo cells a utomatically)”. The ESC can only identify 3S, 4S, 6S and 8S LiPo packs when setting this item to “Auto Calc.” . After you power on the ESC, if the battery voltage is below 1 3.6V, it will be identified as a 3S, if the voltage is fr om 13.6V to 17.6V, it will be identified as a 4S, if the voltage is fr om 17.6V to 26.5V, it will be identified as a 6S, if the voltage is above 26.5V , it will be identified as a 8S.

Note2:

1) This ESC is not intended for 2S operation. Even if you c an set the “LiPo Cells” to 2S, it still does not work.

2) You need to set “LiPo Cells” to “Auto Calc.” and “Cutof f Voltage” to “Disabled” if you use a NiMH pack or a 5S/7S LiPo.