Over-Heat Protection

C=Celsius, F=Fahrenheit

If the function is activated, the output power will be cut-off when the temperature of the ESC or the internal temperature of the sensored brushless motor is up to a factory-preset value for 5 seconds. When the protection happens, the Green LED will flash.

When the ESC is over-heat: The Green LED flashes as “☆-, ☆-, ☆-” (Single flash).

When the motor is over-heat: The Green LED flashes as “☆-☆-, ☆-☆-, ☆-☆-” (Double flash).

Note: The motor over-heat protection function is only available for the sensored brushless motor made by the same manufacturer of the ESC. For motors made by other manufacturers, this function maybe not available or the protection point doesn’t match the design of the ESC, please disable the over-heat protection function in such a case.