ESC Thermal Protection

C=Celsius, F=Fahrenheit

The ESC will automatically cut off the output and the GREEN LED will flash a short, single flash that repeats (☆, ☆, ☆) when the temperature gets up to the value you preset and activates the ESC thermal protection. The output won’t resume until the temperature gets down.

Warning! Never set the ESC Overheat protection to DISABLED unless in some special situations like racing, otherwise you may damage your ESC and even damage your motor.