Boost Timing

Boost Timing is adjustable from 0 degree to 15 degrees, it has three effects:

a)Compatible with different motors. Some motors may function abnormally with the default Boost Timing (0), you need to adjust the timing to a proper degree and then they will work fine.

b)Fine tune the maximum RPM of the motor through adjusting this Boost Timing. The bigger the timing, the higher the RPM, and the more electric energy it will consume.

c)Make the motor operate at the optimum efficiency point through adjusting this Timing.

Attention: After you adjust the Timing, you need to check the actual effect first and then decide if it’s necessary to make the adjustment.

Note: In “Hybrid” mode, 1 degree (of Boost Timing) in setting equals to 2 degrees (of Boost timing) in reality. To be specific, you will actually have 20 degrees of Boost Timing when you set this item to 10 degrees.