Boost Timing

It is effective throughout the entire throttle range and affects the motor speed in the entire track. Please note this refers to the maximum value of the ESC internal timing, the actual timing is always dynamically changed every moment according to the motor RPM.

Timing

The “timing” item is usable for both sensored and sensorless brushless motors. Please select the most suitable timing value according to the motor you are just using. Generally, higher timing value brings out higher power output, but the whole efficiency of the system will be slightly lower down.