Boost Timing
This setting sets the total amount of boost timing added across the boost RPM range.
Options: 0-64 points, with steps of 1
Turbo Timing
This setting sets the total amount of turbo timing that can be applied.
Options: 0-64 points, with steps of 1
WARNING: The following settings are recommendation for 1/10 scale on-road touring cars, and the motor has an initial mechanical timing (also called: Endbell timing) of 0 to 5 Degree. Incorrect Boost and Turbo timing settings will cause ESC or motor burning. Check your motor's instruction for proper gear ratio and start from the suggest timing range as follow. Always remember to monitor your motor and ESC's temperature after one or two minutes's running when using a new faster setting.

motor turns | max Boost timing can do | max Turbo timing can do
3.5T/4.0T | 0 deg | 5 deg
4.5/5.5T | 0 deg | 10 deg
6.5T/7.5T | 5 deg | 10 deg
8.5T/9.5T | 10 deg | 15 deg
10.5T/11.5T | 20 deg | 25 deg
≥13.5T | 30 deg | 25 deg