ESC Thermal Protection

The ESC will cut off the output when its internal temperature goes above the preset value. The GREEN LED will flash slowly to indicate the ESC Thermal Protection is activated. The motor can resume rotation and run at halved power after you first move the throttle stick/trigger back to the Zero-Speed throttle position and then move the throttle stick/trigger to the full throttle position. The ESC will resume normal output after the temperature goes below 80℃ (176℉).