Turbo Activation Method
This defines the activation method for the addition of the turbo timing.
Option 1: “Full Throttle” – Turbo timing is activated only after 100% throttle has been applied, and the full throttle delay (setting 28) is elapsed.
Option 2: “RPM” – Turbo timing is activated only after the Turbo Start RPM (setting 29) is achieved.
Option 3: “Full Throttle and RPM” – This is a combination of option 1 and option 2, where the turbo timing will only active if both the full throttle and RPM conditions are met.