Advanced timing

0deg / 4deg / 8deg / 12deg / *15deg / 18deg / 22deg / 26deg / 30deg / Customized: 0deg~30deg, step: 1 deg
In general, the low timing works fine for most motors. While as great differences exist among motors, so please try different timing(s) to get the best driving effect.
For increasing the speed, you can set the timing higher.
After the timing adjustment, we recommend having a trial on the ground first, and then fly in the sky.