Sensor Mode

Option 1: Full Sensored

After selected this option, your whole power system will work in sensored mode all the time. In this mode, the control feel will be better, the efficiency of the power system will be higher, and the Turbo timing of the ESC can be activated to get the maximum burst power.

Option 2: Sensored/Sensorless Hybrid

The ESC drives the motor in sensored mode during the low-speed start-up process, after that the ESC will switch to driving the motor in sensorless mode. This dual drive mode is applicable to 4WD SCT vehicles using 4 pole motors.

Warning！Do not select this option if you are using a non-Hobbywing matching motor, especially when it’s a 4 pole sensored motor, otherwise you may damage your ESC and motor.