Lipo Cells:

For normal voltage ESC (supports 2-6 cells Lipo), the values are *Auto / 2S / 3S / 4S / 5S / 6S, the default is “Auto”; For high voltage ESC (supports 5-12 cells Lipo), the values are *Auto / 5S / 6S / 8S / 10S / 12S, the default is “Auto”. This programmable item is available for lithium battery. In the startup process, the motor will emits several “Beep-” tones to represent the Lipo cells number, it is helpful for you to check whether it is coincident with the actual battery pack or not.

Note4: If you choose “Auto”, the ESC may mistakenly judge the battery cells when the voltage is less than 3.7V/Cell, so we strongly suggest setting the “Lipo Cells” manually.

Note5: For high voltage ESC (supports 5 to 12 cells Lipo), when the motor emits the “Beep” tones to represents the cells number, a long “Beep—” tone = 5 short “Beep-” tone. So 5S = “Beep—”, 6S = ”Beep—Beep-” (1 long 1 short), 8S=”Beep—Beep-Beep-Beep-” (1 long 3 short), 10S= “Beep—Beep—” (2 long), 12S=”Beep—Beep—Beep-Beep-” (2 long 2 short). While for normal voltage ESC (supports 2 to 6 cells Lipo), we still use 5 short “Beep-” tones to represent 5S lipo, and 6 short “Beep-” tones to represent 6S lipo.