Motor Thermal Protection

C=Celsius, F=Fahrenheit

The motor will automatically cut off the output and the GREEN LED will flash a short, double flash that repeats (☆☆, ☆☆, ☆☆) when the temperature gets up to the value you preset and activates the motor thermal protection. The output won’t resume until the temperature gets down.

Warning! Never set the Motor Overheat Protection to DISABLED unless in some special situations like racing, otherwise you may damage your ESC and even damage your motor. For non-HOBBYWING motor, different thermal sensor may cause the ESC to trigger the Motor Thermal Protection early or later. In this case, please set the Motor Overheat Protection to DISABLED and check the motor temperature with an infrared thermometer (or bare hand if you don’t have the device, but be careful all the time) regularly.