- Software Revision History
- CarESC Revision History
- BoatESC Revision History
- AircraftESC Revision History
- ProgramBox Revision History

Version Number | Type | Release Date | Release Notes
1.0.0 | Final | 06-17-2019 | 1. First release.

Database Version | Type | Release Date | Release Notes
DRIVING_V3.52.04 | Final | 12-23-2015 | 1. Released a new version of firmware "XR-4.1.51" (for XeRun-XR8 PLUS) for better "Punch". 2. Released a new version of firmware "V1_509_No Timing"(for XeRun-XR10 Justock).
DRIVING_V3.52.03 | Final | 10-15-2015 | 1. Released a new version of firmware "XR-4.1.30" (for XeRun-XR8 PLUS) for better "Coast". 2. Released a new version of firmware "B1.20"(for EzRun MAX5) due to hardware update (from HW464SL_KZ1_V1.1 to HW464SL_KZ1_V1.3).
DRIVING_V3.52.02 | Final | 09-01-2015 | 1. Released one version of firmware "XR-4.1.25" for XeRun XR8 PLUS. 2. Released the special firmware for EzRun MAX5 and EzRun MAX6.
DRIVING_V3.52.01 | Final | 07-17-2015 | 1. Released one version of firmware "V3.1_121129_Beta" for XeRun-120A-V3. 2. Released the special firmware "XR-4.1.22" for XeRun XR8 PLUS.
150410 | Final | 04-15-2015 | 1. Released the special firmware for EzRun MAX series of ESCs like MAX8, MAX6, MAX5 and etc. 2. Released new firmware "V1.04_150409" for XeRun-150A-V1, "V1.05_150408" for SCT-PRO. Some improvements have been made as shown below: I. Revised factory default settings and improved the reliability of the product. II. Fixed the "low-voltage cutoff protection gets activated too early" issue when using poor-quality batteries.
140627 | Final | 06-27-2014 | Here we release new firmware "V3.2_140627_Beta" for XeRun-120A-V3 ESCs, this new firmware mainly improved the following aspects: 1. Comparing with the previous version, it can bring better low-speed power while less heat to the motor when activating the Boost & Turbo timing; 2. Fixed the short-time weak brake effects after a quick full brake operation with the option "maximum brake force" set to 75% or above. 3. Solved the cogging issue previously happened to some motors at extremely low throttle with Boost/Turbo Timing activated.
130814 | Final | 11-30-2013 | Here we release new firmware "V103_130806-Beta" for XeRun-150A, XeRun-SCT-PRO, EzRun-150A, EzRun-WP-SC8 ESCs, and following improvements have been made on the former version: 1 Excellent low-speed startup greatly improved the linearity. 2. The acceleration is much quicker than before. The new firmware eliminates the discontinuous speed jump in the old firmware, now the control feeling in sensorless mode is very similar to the control feeling of sensored brushless system. 3 Compatibility with Tenshock sensored motor has been observably improved. 4. Supports motors with higher KV. The new firmware solves the trembling problem occurs to some high RPM multi-poles (>=4 poles) motors at partial throttle. 5. The new firmware is "SAFER" than the old one. a) It doesn’t allow the neutral throttle point to coincide with the full throttle point, while the old firmware allows user to set them to a same point. Therefore, the new firmware eliminates the possibility of unexpected full-speed running when the ESC is switched on. Undoubtedly, it makes the whole system safer for users and crowd nearby. b) When the ESC is switched on, the motor can be started ONLY if the ESC detects the throttle signal is correct and in the neutral range. If the throttle signal is out of the neutral range, then the motor cannot be started. This also makes the entire system more secure for RC car drivers and people close by.
130520 | Final | 05-20-2013 | 1. Database is updated to version 130520 for EzRun-WP-60A and EzRun-WP-80A.
130516 | Final | 05-16-2013 | 1. Database is updated to version 130516, which includes the new firmware "V1.01_130515a_2R" for XeRun-150A and XeRun-SCT-PRO ESCs.
2016 | Final | 04-08-2016 | 1. Added the auto-update function for database. 2. The auto-update function of the old version of App doesn’t work anymore due to website update, so you must install the latest version to have the auto-update function. 3. All the update date of our database versions will be displayed in MM, DD, YY. 4. From now on, the word “Beta” will be added in the version name of all the newly added firmware (if it’s a test version) in database. For example: PB-3.2.24 (Beta)... ("Beta" will be shown in the version name only if the ESC is connected to a LCD program box and a laptop. )
130511 | Final | 05-13-2013 | 1. Database is updated to version 130511, which includes the new firmware for XeRun-150A and XeRun-SCT-PRO ESCs. The firmware increases the sensor siganl tolerance for 4 pole sensored motors and the reliability of the ESC, and the startup of motor becomes more powerful and smoother.
121204 | Final | 12-04-2012 | 1. New firmware for XeRun-V3.
120317 | Final | 04-01-2012 | 1. New firmware for XeRun-V3.
111011 | Final | 10-11-2011 | The Firmware database of the car ESC has been updated to the latest Version 111008. 1. Two versions of firmware named "V3.0_110930_MOD" and "V3.0_110930_STOCK: are available for the following ESCs: XeRun-120A (V2.0), XeRun-60A (V2.0), XeRun-120A (V2.1), XeRun-60A (V2.1), Xtreme STOCK a) "V3.0_110930_MOD" is an improved version of firmware based on "V3.0_110119_MOD"; the new firmware has been updated to improve the fault tolerance of the signal quality of the Hall sensors on the sensor PCB of brushless motors. The old firmware was found to be too sensitive to any small change of the sensor signal, in turn causing the ESC to frequently switch its running mode from sensored to sensorless. The new firmware is not as sensitive as the older version, so the ESC can still operate in sensored mode even if the signal has slight changes in amplitude from small error, that may eventually help Mod motors which have very large current flows which cause the signal on the sensor PCB of the motor to change frequently and result in evitable errors . b) "V3.0_110930_STOCK" is a new version based on "V3.0_110211_STOCK", which has the same improvements as above. 2. New firmware named "V3_508_No Timing" is also applicable to the JUSTOCK ESC. The improvements are as follows: a) For finer adjustment, options under the "Maximum Brake Force" has increased from 4 to 8. b) The new firmware has been updated to improve the fault tolerance of the signal quality of the Hall sensors on the sensor PCB of the brushless sensored motor’s. 3. New firmware named "111011_2R" is applicable for the following ESCs: XeRun-80A, XeRun-150A, XeRun-SCT Pro a) "111011_2R" firmware improves the fault tolerance of the signal quality of the Hall sensors within the sensor board of brushless motors.
1.92 | Final | 03-10-2011 | The latest firmware "110211_stock" is released. Team Hobbywing won the Open Brushless Racing in TITC 2011 with this firmware.
1.92 | Final | 01-19-2011 | Two versions of firmware "V3.0_110119STOCK" and "V3.0_1109119_MOD" are released. Compared with the previous versions like 0518_STOCK, the 3rd generation STOCK firmware "110119_STOCK" has the following advantages: 1. Stronger and quicker acceleration, but the temperature of ESC and motor is even lower than before. 2. Boost Timing and Turbo Timing can be adjusted more smoothly, with the precision of 1 degree per step. 3. Turbo Timing and Boost Timing can be composited to be functional together (Total effective timing is 60 degree). 4. Turbo Timing increasing rate (slope rate) is adjustable. 5. Brake Force is changed from 4 options to 8 options.
1.79 | Final | 09-17-2010 | The new firmware "100912-2R" for XeRun-80A, XeRun-150A, EzRun-SC10, EzRun-SC8 has the following improvements: 1. Fixed the bug that ESC can be shut off for a short time (usually several seconds) caused by thermal protection which is mistakenly activated for some reason. 2. Optimized the switching of “Forward and Reverse” running mode.
1.76 | Final | 07-20-2010 | 1. The new firmware "VER1.0_100715-2R" for XeRun-80A and XeRun-150A ESC eliminates the incompatibility issue when the ESC works with Futaba 4PK system in sensored mode, the reliability of the ESC is also improved.
1.75 | Final | 06-10-2010 | 1. The new firmware "100605" for XeRun-150A/80A significantly improves the low-speed startup and throttle linearity. 2. The new firmware "100528_Mod" for XeRun-120A/60A V2.0 (or later) is suitable for Modified class. The turbo technology is also implemented in this firmware, so the top speed is increased.
1.74 | Final | 05-18-2010 | 1. Added new STOCK firmware "100518STOCK" for XeRun-120A-V2, XeRun-60A-V2. 2. Added new firmware "100324_3R" for XeRun-80A, XeRun-150A, which support the sensored motor more smoothly.
1.72 | Final | 04-26-2010 | 1. Added new STOCK firmware "100422STOCK" for XeRun-120A-V2 and XeRun-60A-V2 ,the Dynamic timing and Turbo Timing are availabe with this firmware.
1.69 | Final | 12-18-2009 | 1. Added new firmware for XeRun-120A-V2, XeRun-60A-V2, XeRun-80A-V1, XeRun-150A-V1 ESCs.
1.65 | Final | 11-19-2009 | 1. New firmware is released for CAR ESCs.
| Final | 10-23-2009 | 1. Added some more programmable items.
| Final | 01-16-2009 | 1. Added new firmware for XeRun-120A-V2. 2. Added new firmware for EzRun-80A/150A.
| Final | 01-07-2009 | 1. Added data-recording function for checking the motor’s operation. 2. Revised the firmware: v090105 to make RC vehicle have higher top speed when using GT ESC(s).
| Final | 01-04-2009 | 1. First release

Firmware Version | Type | Release Date | Release Notes

Database Version | Type | Release Date | Release Notes
FLYING_V3.52.06 | Final | 12-24-2015 | 1. Deleted two versions of outdated firmware for Platinum-HV-V4 ESCs (PL-04.0.00 for PL 160A, PL200-04.0.00 for PL 200A) from the software package.
FLYING_V3.52.05 | Final | 12-18-2015 | 1. Added new firmware "PL-04.0.02" for PLATINUM HV series of aircraft ESCs, which revised the voltage test range.
FLYING_V3.52.04 | Final | 11-18-2015 | 1. Released new firmware "PL200-04.0.01" for “Platinum-200A-HV-V4”. 2. Released new firmware "PL-04.0.01" for Platinum-HV-V4 series of ESCs.
FLYING_V3.52.03 | Final | 09-02-2015 | 1. It can support more Platinum-HV-V4 series of ESCs. 2. It can support more Platinum-V4 series of ESCs.
FLYING_V3.52.02 | Final | 08-07-2015 | 1. It can support the Platinum-100A-HV-V3.
FLYING_V3.52.01 | Final | 07-17-2015 | 1. It can support the Platinum-HV-V4 series of ESCs.
140318 | Final | 03-18-2014 | 1. Upgraded the database for Platinum-V3, Platinum-HV-V3 and LCD Program Box. 1.1 Fixed the bug (operation issue when users factory-reset their ESCs via throttle stick) happens to Platinum-V3 & Platinum-HV-V3 series ESCs. 1.2 Decreased the switching speed, when Platinum-V3 & Platinum-HV-V3 series ESCs were/are in the “governor” mode, to 1.7 seconds. 2. Fixed the bug (multfunction LCD program box is not compatible with car ESCs) exists in firmware "V1.16_131105" and update it to "V1.17_140315". 3. Added the firmware for Platinum-30A-OPTO ESCs into the database.
3.42 | Final | 02-21-2014 | 1. Added database for Platinum-V3, Platinum-HV-V3 and LCD Program Box.
3.3 | Final | 05-13-2013 | 1. Added the firmware “PROGRAMECARD / HW310_V2.1 / ‘V1.14_130508’" for LCD Program Box.
3.1 | Final | 12-04-2012 | 1. Added the firmware “PROGRAMECARD / HW310_V2.1 / ‘V1.12_120426’” for LCD Program Box.
3.0 | Final | 04-01-2012 | 1. Released new firmware for for all ESCs.
1.19 | Final | 09-21-2011 | 1. Upgraded the firmware “V1.08_101106_U_a” for PL120A-HV ESC, now the firmware is compatible with V-bar & Hyperion emeter (V2) tachometer RPM sensor.
1.18 | Final | 08-31-2011 | 1. Upgraded the firmware for Platinum series of ESCs. Now the firmware is only applicable for PL40A-PRO, PL60A-PRO, PL80A-PRO, PL100A-PRO, and PL120A-HV.
1.17 | Final | 01-19-2011 | 1. Upgraded the firmware for 2In1 LCD Program Box.
1.15 | Final | 11-06-2010 | 1. Upgraded the firmware for Platinum series of ESCs. Now the firmware is only applicable for PL40A-PRO, PL60A-PRO, PL80A-PRO, and PL100A-PRO.
1.14 | Final | 05-12-2010 | 1. Upgraded the firmware for Platinum series of ESCs. Now the firmware is only applicable for PL40A-PRO, PL60A-PRO, PL80A-PRO, and PL100A-PRO. 2. Upgraded the firmware for the 2In1 LCD Program Box. Now more programmable items or parameters will be displayed when programming XeRun series of Car ESCs (in STOCk mode) with this LCD Program Box.
1.13 | Final | 04-22-2010 | 1. Upgraded the firmware for Platinum series of ESCs. Now the firmware is only applicable for PL40A-PRO, PL60A-PRO, PL80A-PRO, and PL100A-PRO.
1.10 | Final | 12-24-2009 | 1. If users program their ESCs during the running, then they should reset the ESCs before driving motors.
1.09 | Final | 10-23-2009 | 1. First release

Firmware Version | Type | Release Date | Release Notes
PB-3.2.31 | Final | 10-28-2016 | 1. Optimize the performance of the LCD program box.
PB-3.2.30 | Final | 08-15-2016 | 1. It can support XeRun XR10 PRO ESCs to have more programmable items.
PB-3.2.28 | Final | 06-04-2016 | 1. It can support more XeRun XR10 PRO series of ESCs. 2. It supports the LCD program box to display temperatures in Fahrenheit degrees and capacitor temperature also in Fahrenheit degrees for Platinum V4 series & Platinum HV V4 series of aircraft ESCs.
PB-3.2.25 | Final | 04-08-2016 | 1. It can support the programming of EzRun MAX10. 2. Fixed the display issue after connected the XR8 ESC to a LCD program box for ESC programming.
PB-3.2.22 | Final | 11-18-2015 | 1. It can support the programming of Seaking Pro 160A.
PB-3.2.21 | Final | 10-15-2015 | 1.Revised the firmware for ensuring BEC voltages displayed on the LCD program box equal to the actual BEC voltages of ESCs.
PB-3.2.20 | Final | 09-02-2015 | 1. It can support more EzRun MAX V3 series of car ESCs and Platinum LV V4 series of aircraft ESCs.
PB-3.2.19 | Final | 07-17-2015 | 1. It can supports EzRun MAX V3 series of car ESCs, PLATINUM HV V4 series of aircraft ESCs, and XeRun XR8 series of car ESCs.
1.18_150114 | Final | 04-15-2015 | 1. It can support EzRun MAX V3 series of car ESCs and PLATINUM V4 series of aircraft ESCs.