Boost Slope (BT Slope)
This setting controls how the boost timing is applied within the RPM range. There are two options for this setting.
Option 1: “Linear” – This applies the boost in a linear manner within the RPM Range. The ESC calculates the rate of addition of boost, based off of Setting 21, 22 & 23.
Option 2: “Custom” – This allows for a non-linear addition of Boost timing within the RPM range. The boost can be applied in multiple increasing steps throughout the range.