Lipo Cells:

Platinum-V3:
Auto calculation / 1 cells / 2 cells / 3 cells / 4 cells / 5 cells / 6 cells
Platinum-HV-V3:
Auto calculation / 1 cells / 2 cells / 3 cells / 4 cells / 5 cells / 6 cells
The parameter is valid only when the battery pack is LiPo. After powered on, the ESC will make the motor beep the amount of cells in your LiPo pack according to auto-detection or cell count manually set.
For Platinum-50A-V3,
Platinum-100A-V3 ESCs, the range which can be auto-calculated or manually set is 2~6S; if exceeds, the system will warn.
For Platinum-80A-HV-V3 ESCs, the range which can be auto-calculated or manually set is 5~12S; if exceeds, the system will warn.