HobbyWing

Drive Mode

Option 1: Hybrid

The ESC drives the motor in sensored mode during the low-speed start-up process, after that the ESC will switch to driving the motor in sensorless mode.

Option 2: Full Sensored

You can select this option only when using a HOBBYWING matching motor (that means HOBBYWING new 1:8th motor without Hall sensor interference), the control feeling will be better, the efficiency of the power system will be higher, and the turbo timing of the ESC can be activated to get the maximum burst power.

Warning!

1) Do not select this option if you use a non-HOBBYWING matching motor, especially when it’s a 4 pole sensored motor, otherwise you may damage the ESC and the motor.

2) If you select this option but you forget to plug the motor sensor cable in or you connect your ESC to a sensorless motor, then the ESC will be unable to drive the motor.