HobbyWing

Low-voltage Cutoff Threshold

Off / Low / *Middle / High / Customized: 2.8V~25.2V，Step: 0.1V
1, When set as “LiPo battery”, the ESC will automatically calculate the cutoff threshold of the battery pack according to the amount of LiPo cells. The low / middle / high cutoff voltage per cell is 2.85V / 3.15V /
3.30V. For example, when using a 3S LiPo, if set the cutoff voltage as “middle”, the cutoff threshold of this battery pack should be 3.15×3=9.45V.
2, When set as “NiMH battery”, then the low / middle / high cutoff voltage is 50% / 62.5% / 75% of the initial input voltage (at boot/starting up) . For example, when using a 6-cell NiMH battery pack,
the voltage at starting up is 1.44×6=8.64V; and if set the cutoff threshold as “low”, the cutoff threshold of this battery pack should be 8.64×50%=4.3V.
3, When set as “Customized: 2.8V~25.2V”, the cutoff threshold of the battery pack can be precisely set (the precision can reach 0.1V). But you need a LCD program box (optional accessory) or USB cable on
the LCD program box to connect the ESC to a PC, then set relevant parameters via a special program (Hobbywing USB Link Software).