HobbyWing

Lipo Cells

We strongly recommend setting this item manually instead of using the default setting “Auto Calc. (which means auto calculate the Lipo cells)”. The ESC can only identify 3S, 4S and 6S LiPo packs when setting this item to “Auto Calc.”. After you power on the ESC, if the battery voltage is below 13.2V, it will be identified as a 3S, if the voltage is from 13.2V to 17.6V, it will be identified as a 4S, if the voltage is above 17.6V, and it will be identified as a 6S.

Note 2:

1）This ESC is not intended for 2S operation. Even if you can set the “LiPo Cells” to 2S, it still does not work.

2）You need to set “LiPo Cells” to “Auto Calc.” and “Cutoff Voltage” to “None” if you use a NiMH pack or a 5S LiPo.