HobbyWing

Motor Overheat Protection

C=Celsius, F=Fahrenheit

If this function is selected, the output power will be cut-off if the internal temperature of the Motor hits the set level for 5 seconds. When the protection activates, the LED will flash in the following sequence “☆-☆-, ☆-☆-, ☆-☆-” (Double flash).
Options: 85°C/185°F , 105°C/221°F , 125°C/257°F , Disabled

Note: The motor overheat function is only available for sensored brushless motors made by HOBBYWING. For other manufacturers’ motors, this function may not be available, or the sensor may not match the ESC design. For such a case, please disable this function.