HobbyWing

Boost Start RPM
This setting defines the RPM at which the boost timing is started to be added.
Options: 1,000rpm – 35,000rpm, with steps of 500rpm.
Boost End RPM
This setting defines the RPM at which the full level of boost timing is applied.
Options: 3,000rpm – 60,000rpm, with steps of 500rpm.
For example:
Boost timing = 5, boost start rpm = 10000, boost end rpm = 15000, the dynimac timing is follow table:

motor RPM in practice | Boost timing in practice
<10000 | 0 deg
10001-11000 | 1 deg
11001-12000 | 2 deg
12001-13000 | 3 deg
13001-14000 | 4 deg
14001-15000 | 5 deg
>15000 | 5 deg