Throttle Input Curve
This setting is used to define the input throttle curve into the ESC.
Option 1: “Linear” – This is where the forward throttle position of the transmitter directly relates to the forward throttle position into the ESC.
Option 2: “Custom” – This allows for a multi-step setting to the forward throttle. This differs from exponential on the transmitter, in that the forward throttle input into the ESC can be defined in multiple increasing steps.