Motor Rotate

Pull the throttle trigger with the motor shaft faces you, the motor spins counter clockwise if this item is set to CCW; the motor spins clockwise if it’s set to CW. In general, the vehicle goes forward when the motor rotates counter clockwise. However, some chassis manufacturers design their products base on the completely different theories, so your vehicle may go backward when the motor spins counter clockwise. In that case, you need to set this item to CW instead.